Installed berryboot

<https://www.howtogeek.com/141325/how-to-multi-boot-your-raspberry-pi-with-berryboot/>

<https://www.berryterminal.com/doku.php/berryboot#berryboot_v20_-_bootloaderuniversal_operating_system_installer>

Installed Raspbian stretch lite minimal - terminal only with berryboot setup

* 1. sudo apt-get update
  2. sudo apt-get upgrade
  3. sudo raspi-config
     1. fix keyboard layout
     2. enable i2c
  4. sudo apt --fix-broken install (due to error messages)
  5. sudo apt-get install python-smbus
  6. sudo apt-get install i2c-tools

install circuit python libraries from adafruit

* 1. <https://learn.adafruit.com/circuitpython-on-raspberrypi-linux/installing-circuitpython-on-raspberry-pi>
  2. sudo apt-get install python3-pip
  3. sudo pip3 install --upgrade setuptools

sudo pip3 install --upgrade setuptools

If above doesn't work try

sudo apt-get install python3-pip